|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SJLT WOVENS PVT LTD**  **GREIGE FABRIC PURCHASE ORDER** | | | | | | | | | | | | |
| **SJLT WOVENS PVT LTD** | | | | | | | | | | |  | |
| NH-7, Namakkal Karur Main Road, Pillaikalathur, Paramathi,  Namakkal, Tamil Nadu – 637207  Email id: [weaving@sjlt.in](mailto:weaving@sjlt.in)  Phone No: +91 9500988297 | | | | | | GSTIN: 33ABDCS6945H1Z6  CIN No: U17100TN2020PTC135456 | | | | |
|  | | | | | | | | | | | | |
| PO Date: | | | | | | | Payment Terms: | | | | | |
| PO Number: | | | | | | | Price Basis: | | | | | |
|  | | | | | | | Delivery Date: | | | | | |
| Supplier Name:  Address:  Contact Person:  Contact No:  Supplier GSTIN: | | | | | | | Delivery Address: | | | | | |
|  | | | | | | | | | | | | |
| **SNo** | **HSN Code** | **TC** | | **Yarn Count** | **Construction** | | | **Qty** | **Rate** | | | **Total amount** |
|  |  |  | |  |  | | |  |  | | |  |
|  |  |  | |  |  | | |  |  | | |  |
|  |  |  | |  |  | | |  |  | | |  |
|  | | | | | | | | | | | | |
| **Total Amount Before Tax:** | | | | | | | | | |  | | |
| IGST:  CGST:  SGST:  **Total GST:** | | | | | | | | | | xxx  xxx  xxx  xxx | | |
| **Total Value:** | | | | | | | | | |  | | |
| **Amount in words:** | | |  | | | | | | | | | |
| **Delivery Schedule:** | | | | | | | | | | | | |
| **Terms and Condition:**   1. Must deliver within ship window else PO will get cancelled 2. Pre-Production samples must be approved before bulk production 3. Original Invoices to be sent to office address only 4. All payment subject to goods shipped as per our product specification and quality parameter 5. Weaver will be entirely responsible for post processing defects which are not visible to the naked eye and can only be detected by Labs 6. All disputes subject to Namakkal Jurisdiction Only | | | | | | | | | | | | |
| Prepared By | | | | Checked By | | | | For SJLT WOVENS PVT LTD  Authorised Signatory | | | | |

**ANNEXURE**

**Quality Standards:**

1. Fabric will be in roll form securely packed with LDPE sheet and HDPE woven sheet.
2. Roll length will be 95% 350 metres and above, 5% 100 metres and above.
3. Fabric will be as per American 4 point system. Maximum permissible points will be 16 points per 100 linear metre.
4. Cuttable defects must be tagged.
5. Maximum 3 cuttable faults will allowed per 100 metres.
6. No continuous fault will be accepted above 3 metres.
7. Fabric will inspected by our QC.
8. First metre sample must be sent to our technical team for approval before bulk production.
9. Fabric inspection will be done by our QC inspector after preliminary inspection and mending by your quality team.
10. Fabric will be as per the peg plan, if provided.
11. Zero Tolerance in Yarn Count, Thread count &width.